Altium Designer Pick and Place Locations
H:\Projects\Signetik\Signetik-DEV-A1\trunk\cellular-breakout-adapter\Project Outputs for cellular-breakout-adapter\[3] Assembly_REV4\Pick Place\cellular-breakout-adapter_REV4_Generates pick and place files.txt

========================================================================================================================
File Design Information:

Date:       13/02/21
Time:       04:11
Revision:   Not in VersionControl
Variant:    No variations
Units used: mil

Designator Comment                        Layer    Footprint                                Center-X(mil) Center-Y(mil) Rotation Description                                                                                                                                               
J6         "CONN HEADER VERT 6POS 2.54MM" TopLayer Harwin_M20-9980345_0                     36.026        644.951       180      "Connector Header Through Hole 6 position 0.100" (2.54mm)"                                                                                                
C5         1uF                            TopLayer 0603_CAP_NP                              177.136       948.344       90       "CAP CER 1UF 25V X7R 0603"                                                                                                                                
C3         1uF                            TopLayer 0603_CAP_NP                              45.026        860.457       0        "CAP CER 1UF 25V X7R 0603"                                                                                                                                
C2         1uF                            TopLayer 0603_CAP_NP                              45.026        795.951       0        "CAP CER 1UF 25V X7R 0603"                                                                                                                                
U3         CP2105-F01-GMR                 TopLayer Silicon_Labs_CP2105-F01-GMR_IPC_A        36.026        1036.479      90       "USB Bridge, USB to UART USB 2.0 UART Interface 24-QFN (4x4)"                                                                                             
P4         M20-9990246                    TopLayer Male_1X2_2.54P_TH                        -1471.864     1014.951      90       "Connector Header Through Hole 2 position 0.100" (2.54mm)"                                                                                                
P8         M20-9990246                    TopLayer Male_1X2_2.54P_TH                        -1342.864     1015.951      90       "Connector Header Through Hole 2 position 0.100" (2.54mm)"                                                                                                
R9         4.7k                           TopLayer 0402_RES                                 177.136       1051.792      90       "Resistor 4.7k Ohm ±1% 0.063W 0402"                                                                                                                       
R8         1k                             TopLayer 0402_RES                                 -125.000      1077.707      180      "RES SMD 1K OHM 1% 1/16W 0402"                                                                                                                            
R7         1k                             TopLayer 0402_RES                                 -125.000      1046.322      180      "RES SMD 1K OHM 1% 1/16W 0402"                                                                                                                            
R6         "0.5, 1W"                      TopLayer 2512_RES                                 -346.864      902.951       180      "500 mOhms ±1% 1W Chip Resistor 2512 (6432 Metric) Anti-Sulfur, Automotive AEC-Q200, Current Sense, Moisture Resistant, Pulse Withstanding Metal Element" 
P9         CON3_2.54mm_VERT_TH            TopLayer Male_1X3_2.54P_TH                        533.136       626.951       180      "Connector 3 Pin 2.54mm Vertical TH"                                                                                                                      
R13        1k                             TopLayer 0402_RES                                 -1227.864     936.951       270      "RES SMD 1K OHM 1% 1/16W 0402"                                                                                                                            
R12        1k                             TopLayer 0402_RES                                 -1102.531     936.951       270      "RES SMD 1K OHM 1% 1/16W 0402"                                                                                                                            
U1         TPD4S012                       TopLayer PSON_6_P50                               295.136       1132.951      270      "IC 4 Channel ESD With Clamp 6SON"                                                                                                                        
P7         CON3_2.54mm_VERT_TH            TopLayer Male_1X3_2.54P_TH                        432.369       938.951       90       "Connector 3 Pin 2.54mm Vertical TH"                                                                                                                      
P6         M20-9990246                    TopLayer Male_1X2_2.54P_TH                        -602.864      1057.951      180      "Connector Header Through Hole 2 position 0.100" (2.54mm)"                                                                                                
P5         M20-9990246                    TopLayer Male_1X2_2.54P_TH                        -360.864      1057.951      180      "Connector Header Through Hole 2 position 0.100" (2.54mm)"                                                                                                
J5         10118194-0001LF                TopLayer USB_B_RA_SMT-TH_10118194-0001LF(Primary) 293.506       1273.802      180      "USB - micro B USB 2.0 Receptacle Connector 5 Position Surface Mount, Right Angle; Through Hole"                                                          
J4         CON14                          TopLayer Male_1X14_2.54P_TH                       -628.864      1263.951      180      "Connector Header Through Hole 14 position 0.100" (2.54mm)"                                                                                               
D8         Orange                         TopLayer LED_0603/1608_YELLOW                     -1227.864     1043.951      90       "Orange 602nm LED Indication - Discrete 2.1V 0603 (1608 Metric)"                                                                                          
D7         Orange                         TopLayer LED_0603/1608_YELLOW                     -1102.531     1043.951      90       "Orange 602nm LED Indication - Discrete 2.1V 0603 (1608 Metric)"                                                                                          
Q2         DMN1150UFL3                    TopLayer X2DFN35P100X130X35-6N                    -934.864      1160.951      270      "Dual N-Channel FET"                                                                                                                                      
C4         0.1uF                          TopLayer 0402_CAP_NP                              293.136       1067.951      360      "CAP CER 0.1UF 25V X7R 0402"                                                                                                                              
C8         0.1uF                          TopLayer 0603_CAP_NP                              248.136       948.344       90       "Ceramic Cap 0.10µF ±10% 50V X7R 0603"                                                                                                                    
J2         NRPN101BFCN-RC                 TopLayer Female_1x10_VER_TH_2mm                   -1323.864     211.744       360      "10 Position Header Connector Through Hole"                                                                                                               
J1         PJ-002AH                       TopLayer CUI_PJ-002AH_0                           641.616       999.841       90       "Power Barrel Connector Jack 2.10mm ID (0.083"), 5.50mm OD (0.217") Through Hole, Right Angle"                                                            
R5         0                              TopLayer 1210_RES                                 -290.365      633.074       90       "RES SMD 0.0 OHM JUMPER 0.5W 1210"                                                                                                                        
R4         1k                             TopLayer 0402_RES                                 -977.197      936.951       270      "RES SMD 1K OHM 1% 1/16W 0402"                                                                                                                            
R3         1k                             TopLayer 0402_RES                                 -851.864      936.951       270      "RES SMD 1K OHM 1% 1/16W 0402"                                                                                                                            
R2         470                            TopLayer 0402_RES                                 784.136       784.951       270      "RES SMD 470 OHM 1% 1/16W 0402"                                                                                                                           
R1         750                            TopLayer 0402_RES                                 594.136       784.951       90       "RES SMD 750 OHM 1% 1/16W 0402"                                                                                                                           
P3         "DNP M20-9990246"              TopLayer Male_1X2_2.54P_TH                        854.136       626.951       180      "Connector Header Through Hole 2 position 0.100" (2.54mm)"                                                                                                
MT6        MTHole                         TopLayer SMTSO-080-2ET                            -1428.888     -308.422      0        "Surface mount ReelFast® microPEM® (Type SMTSO™) fasteners for compact electronic assemblies attach to P.C. Boards for nut/standoff applications."        
MT5        MTHole                         TopLayer SMTSO-080-2ET                            -1417.077     723.074       0        "Surface mount ReelFast® microPEM® (Type SMTSO™) fasteners for compact electronic assemblies attach to P.C. Boards for nut/standoff applications."        
MT4        MTHole                         TopLayer SMTSO-080-2ET                            -680.856      -308.422      0        "Surface mount ReelFast® microPEM® (Type SMTSO™) fasteners for compact electronic assemblies attach to P.C. Boards for nut/standoff applications."        
MT3        MTHole                         TopLayer SMTSO-080-2ET                            -692.667      723.074       0        "Surface mount ReelFast® microPEM® (Type SMTSO™) fasteners for compact electronic assemblies attach to P.C. Boards for nut/standoff applications."        
J3         NRPN101BFCN-RC                 TopLayer Female_1x10_VER_TH_2mm                   -458.864      212.744       360      "10 Position Header Connector Through Hole"                                                                                                               
D4         Orange                         TopLayer LED_0603/1608_YELLOW                     -977.197      1043.951      270      "Orange 602nm LED Indication - Discrete 2.1V 0603 (1608 Metric)"                                                                                          
D3         Orange                         TopLayer LED_0603/1608_YELLOW                     -851.864      1043.951      270      "Orange 602nm LED Indication - Discrete 2.1V 0603 (1608 Metric)"                                                                                          
D2         GRN                            TopLayer APTD1608LZGCK                            668.136       762.951       270      "Green 525nm LED Indication - Discrete 2.65V 2mA 0603 (1608 Metric)"                                                                                      
D1         RED                            TopLayer LED_0603/1608_RED                        852.136       762.951       270      "Red 638nm LED Indication - Discrete 1.8V 0603 (1608 Metric)"                                                                                             
C1         10uF                           TopLayer 0603_CAP_NP                              459.490       743.951       180      "CAP CER 10UF 10V X5R 0603"                                                                                                                               
P2         DF40C-20DP-0.4V(51)            TopLayer CONN20_6P6X2P9_HEADER                    -1054.864     -312.358      0        "CONN HDR 20POS 0.4MM SMD GOLD"                                                                                                                           
P1         DF40HC(2.5)-20DS-0.4V(51)      TopLayer CONN20_6P6X2P9_2.5MM                     374.010       -3.934        360      "CONN RCPT 20POS 0.4MM SMD GOLD"                                                                                                                          
